# 3D printable case for PiKVM v3.2 HAT - PiKVM Handbook
Open and cheap DIY IP-KVM on Raspberry Pi
Author: Maxim Devaev

Skip to content

# 3D printable case for PiKVM v3.2 HAT

When printing the case, you can choose the following options:

- The presence or absence of an OLED screen (used to display the IP address and other information).
- The presence or absence of holes for the AUM v3.3 (Advanced USB Module, most likely you don't have it).

Also take a look at the PCI bracket for ATX adapter board.

## Buy options

- Small 5v fan strongly recommended to avoid overheating in the case.
- I2C OLED screen.

## Building

## Parts

### The front part

Choose ONE of them.

Variant | Description
--- | ---
| The front part of the case WITHOUT a hole for the OLED
| The front part of the case with a hole for installing the OLED

### The back part

Choose ONE of them.

Variant | Description
--- | ---
| The back part of the case WITHOUT AUM holes
| The back part of the case for installing the AUM

### Spacers

Type | Description
--- | ---
| 6.2mm spacer, required TWO pieces
| 2mm spacer required TWO without AUM or ONE for AUM
| 1mm spacer required ONE for AUM only
| Low spacer required ONE